hlsl.struct.split.array.geom
Shader version: 500
invocations = -1
max_vertices = 4
input primitive = points
output primitive = triangle_strip
0:? Sequence
0:13  Function Definition: @main(u1[1];struct-PSInput-vf4-vf2-vf3-u11; ( temp void)
0:13    Function Parameters: 
0:13      'v' ( in 1-element array of uint)
0:13      'OutputStream' ( out structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:?     Sequence
0:16      Sequence
0:16        move second child to first child ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:16          'Out' ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:16          Constant:
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0 (const uint)
0:18      Sequence
0:18        move second child to first child ( temp int)
0:18          'x' ( temp int)
0:18          Constant:
0:18            0 (const int)
0:18        Loop with condition tested first
0:18          Loop Condition
0:18          Compare Less Than ( temp bool)
0:18            'x' ( temp int)
0:18            Constant:
0:18              2 (const int)
0:18          Loop Body
0:19          Sequence
0:19            move second child to first child ( temp int)
0:19              'y' ( temp int)
0:19              Constant:
0:19                0 (const int)
0:19            Loop with condition tested first
0:19              Loop Condition
0:19              Compare Less Than ( temp bool)
0:19                'y' ( temp int)
0:19                Constant:
0:19                  2 (const int)
0:19              Loop Body
0:20              move second child to first child ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:20                indirect index ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:20                  indirect index ( temp 3-element array of structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:20                    'Verts' ( temp 2-element array of 3-element array of structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:20                    'x' ( temp int)
0:20                  'y' ( temp int)
0:20                'Out' ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:19              Loop Terminal Expression
0:19              Pre-Increment ( temp int)
0:19                'y' ( temp int)
0:18          Loop Terminal Expression
0:18          Pre-Increment ( temp int)
0:18            'x' ( temp int)
0:13  Function Definition: main( ( temp void)
0:13    Function Parameters: 
0:?     Sequence
0:13      move second child to first child ( temp 1-element array of uint)
0:?         'v' ( temp 1-element array of uint)
0:?         'v' (layout( location=0) in 1-element array of uint)
0:13      Function Call: @main(u1[1];struct-PSInput-vf4-vf2-vf3-u11; ( temp void)
0:?         'v' ( temp 1-element array of uint)
0:?         'OutputStream' ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:?   Linker Objects
0:?     'v' (layout( location=0) in 1-element array of uint)
0:?     'OutputStream' (layout( location=0) out structure{ temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})


Linked geometry stage:


Shader version: 500
invocations = 1
max_vertices = 4
input primitive = points
output primitive = triangle_strip
0:? Sequence
0:13  Function Definition: @main(u1[1];struct-PSInput-vf4-vf2-vf3-u11; ( temp void)
0:13    Function Parameters: 
0:13      'v' ( in 1-element array of uint)
0:13      'OutputStream' ( out structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:?     Sequence
0:16      Sequence
0:16        move second child to first child ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:16          'Out' ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:16          Constant:
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0.000000
0:16            0 (const uint)
0:18      Sequence
0:18        move second child to first child ( temp int)
0:18          'x' ( temp int)
0:18          Constant:
0:18            0 (const int)
0:18        Loop with condition tested first
0:18          Loop Condition
0:18          Compare Less Than ( temp bool)
0:18            'x' ( temp int)
0:18            Constant:
0:18              2 (const int)
0:18          Loop Body
0:19          Sequence
0:19            move second child to first child ( temp int)
0:19              'y' ( temp int)
0:19              Constant:
0:19                0 (const int)
0:19            Loop with condition tested first
0:19              Loop Condition
0:19              Compare Less Than ( temp bool)
0:19                'y' ( temp int)
0:19                Constant:
0:19                  2 (const int)
0:19              Loop Body
0:20              move second child to first child ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:20                indirect index ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:20                  indirect index ( temp 3-element array of structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:20                    'Verts' ( temp 2-element array of 3-element array of structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:20                    'x' ( temp int)
0:20                  'y' ( temp int)
0:20                'Out' ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:19              Loop Terminal Expression
0:19              Pre-Increment ( temp int)
0:19                'y' ( temp int)
0:18          Loop Terminal Expression
0:18          Pre-Increment ( temp int)
0:18            'x' ( temp int)
0:13  Function Definition: main( ( temp void)
0:13    Function Parameters: 
0:?     Sequence
0:13      move second child to first child ( temp 1-element array of uint)
0:?         'v' ( temp 1-element array of uint)
0:?         'v' (layout( location=0) in 1-element array of uint)
0:13      Function Call: @main(u1[1];struct-PSInput-vf4-vf2-vf3-u11; ( temp void)
0:?         'v' ( temp 1-element array of uint)
0:?         'OutputStream' ( temp structure{ temp 4-component vector of float Pos,  temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})
0:?   Linker Objects
0:?     'v' (layout( location=0) in 1-element array of uint)
0:?     'OutputStream' (layout( location=0) out structure{ temp 2-component vector of float TexCoord,  temp 3-component vector of float TerrainPos,  temp uint VertexID})

// Module Version 10000
// Generated by (magic number): 80001
// Id's are bound by 77

                              Capability Geometry
               1:             ExtInstImport  "GLSL.std.450"
                              MemoryModel Logical GLSL450
                              EntryPoint Geometry 4  "main" 66 76
                              ExecutionMode 4 InputPoints
                              ExecutionMode 4 Invocations 1
                              ExecutionMode 4 OutputTriangleStrip
                              ExecutionMode 4 OutputVertices 4
                              Source HLSL 500
                              Name 4  "main"
                              Name 14  "PSInput"
                              MemberName 14(PSInput) 0  "Pos"
                              MemberName 14(PSInput) 1  "TexCoord"
                              MemberName 14(PSInput) 2  "TerrainPos"
                              MemberName 14(PSInput) 3  "VertexID"
                              Name 19  "@main(u1[1];struct-PSInput-vf4-vf2-vf3-u11;"
                              Name 17  "v"
                              Name 18  "OutputStream"
                              Name 21  "Out"
                              Name 30  "x"
                              Name 41  "y"
                              Name 54  "Verts"
                              Name 64  "v"
                              Name 66  "v"
                              Name 68  "OutputStream"
                              Name 69  "param"
                              Name 71  "param"
                              Name 74  "PSInput"
                              MemberName 74(PSInput) 0  "TexCoord"
                              MemberName 74(PSInput) 1  "TerrainPos"
                              MemberName 74(PSInput) 2  "VertexID"
                              Name 76  "OutputStream"
                              Decorate 66(v) Location 0
                              Decorate 76(OutputStream) Location 0
               2:             TypeVoid
               3:             TypeFunction 2
               6:             TypeInt 32 0
               7:      6(int) Constant 1
               8:             TypeArray 6(int) 7
               9:             TypePointer Function 8
              10:             TypeFloat 32
              11:             TypeVector 10(float) 4
              12:             TypeVector 10(float) 2
              13:             TypeVector 10(float) 3
     14(PSInput):             TypeStruct 11(fvec4) 12(fvec2) 13(fvec3) 6(int)
              15:             TypePointer Function 14(PSInput)
              16:             TypeFunction 2 9(ptr) 15(ptr)
              22:   10(float) Constant 0
              23:   11(fvec4) ConstantComposite 22 22 22 22
              24:   12(fvec2) ConstantComposite 22 22
              25:   13(fvec3) ConstantComposite 22 22 22
              26:      6(int) Constant 0
              27: 14(PSInput) ConstantComposite 23 24 25 26
              28:             TypeInt 32 1
              29:             TypePointer Function 28(int)
              31:     28(int) Constant 0
              38:     28(int) Constant 2
              39:             TypeBool
              49:      6(int) Constant 3
              50:             TypeArray 14(PSInput) 49
              51:      6(int) Constant 2
              52:             TypeArray 50 51
              53:             TypePointer Function 52
              60:     28(int) Constant 1
              65:             TypePointer Input 8
           66(v):     65(ptr) Variable Input
     74(PSInput):             TypeStruct 12(fvec2) 13(fvec3) 6(int)
              75:             TypePointer Output 74(PSInput)
76(OutputStream):     75(ptr) Variable Output
         4(main):           2 Function None 3
               5:             Label
           64(v):      9(ptr) Variable Function
68(OutputStream):     15(ptr) Variable Function
       69(param):      9(ptr) Variable Function
       71(param):     15(ptr) Variable Function
              67:           8 Load 66(v)
                              Store 64(v) 67
              70:           8 Load 64(v)
                              Store 69(param) 70
              72:           2 FunctionCall 19(@main(u1[1];struct-PSInput-vf4-vf2-vf3-u11;) 69(param) 71(param)
              73: 14(PSInput) Load 71(param)
                              Store 68(OutputStream) 73
                              Return
                              FunctionEnd
19(@main(u1[1];struct-PSInput-vf4-vf2-vf3-u11;):           2 Function None 16
           17(v):      9(ptr) FunctionParameter
18(OutputStream):     15(ptr) FunctionParameter
              20:             Label
         21(Out):     15(ptr) Variable Function
           30(x):     29(ptr) Variable Function
           41(y):     29(ptr) Variable Function
       54(Verts):     53(ptr) Variable Function
                              Store 21(Out) 27
                              Store 30(x) 31
                              Branch 32
              32:             Label
                              LoopMerge 34 35 None
                              Branch 36
              36:             Label
              37:     28(int) Load 30(x)
              40:    39(bool) SLessThan 37 38
                              BranchConditional 40 33 34
              33:               Label
                                Store 41(y) 31
                                Branch 42
              42:               Label
                                LoopMerge 44 45 None
                                Branch 46
              46:               Label
              47:     28(int)   Load 41(y)
              48:    39(bool)   SLessThan 47 38
                                BranchConditional 48 43 44
              43:                 Label
              55:     28(int)     Load 30(x)
              56:     28(int)     Load 41(y)
              57: 14(PSInput)     Load 21(Out)
              58:     15(ptr)     AccessChain 54(Verts) 55 56
                                  Store 58 57
                                  Branch 45
              45:                 Label
              59:     28(int)     Load 41(y)
              61:     28(int)     IAdd 59 60
                                  Store 41(y) 61
                                  Branch 42
              44:               Label
                                Branch 35
              35:               Label
              62:     28(int)   Load 30(x)
              63:     28(int)   IAdd 62 60
                                Store 30(x) 63
                                Branch 32
              34:             Label
                              Return
                              FunctionEnd
